filename-field

Mapping VC-6 into the MXF Generic Container

Warning

This document is an unpublished, confidential work under development and shall not be referred to as a SMPTE Standard, Recommended Practice, or Engineering Guideline. It is distributed for review and comment; distribution does not constitute publication. Recipients of this document are strongly encouraged to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

**Information for document editors**

* This template is designed to focus on content and not on style. This means that editors should:
  + Refrain from adding styles inline unless absolutely necessary
  + Refrain from modifying styles unless absolutely necessary
  + Use the sample styles & layouts for all headings, figures, tables and math
  + Use the supplied auto numbering styles for headings and annexes
* In the event that the content cannot be adequately expressed using this template, contact SMPTE HQ.
  + The blue text (like this sentence) is editing information or boilerplate. This is information used by SMPTE HQ for publication and should not be changed by the author.
  + The document editor must fill in the fields in black before submitting it to the Drafting Group.
  + The red text (like this sentence) is helpful information that is not part of the final document. This information **shall be deleted** prior to FCD Ballot.
  + The last page of this document has editing hints and a list of useful reference documents. :::

Project Group: *TBD - DG-VC-6-MXF*

Project Technology Committee: *TC 31FS*

Document type: *ST*

Document state: *WD*

Project chair(s): *SMPTE Group chair*

Document editor(s): *Bruce Devlin*

Document number: *xxxx*

Document title: *Mapping VC-6 into the MXF Generic Container*

**Title Page**

This page will be provided by SMPTE HQ Staff.

See AG-16 clause 3.1 (Title Page), and ISO Directive Part 2 clause 11 (Title).

Proposed SMPTE Standard

This document is subject to change Copyright (C) 2020 SMPTE All rights reserved

# Foreword

See AG-16 3.2 (Foreword), and ISO Directive Part 2 clause 12 (Foreword).

SMPTE (the Society of Motion Picture and Television Engineers) is an internationally-recognized standards developing organization. Headquartered and incorporated in the United States of America, SMPTE has members in over 80 countries on six continents. SMPTE“s Engineering Documents, including Standards, Recommended Practices, and Engineering Guidelines, are prepared by SMPTE”s Technology Committees. Participation in these Committees is open to all with a bona fide interest in their work. SMPTE cooperates closely with other standards-developing organizations, including ISO, IEC and ITU. SMPTE Engineering Documents are drafted in accordance with the rules given in its Standards Operations Manual. This SMPTE Engineering Document was prepared by Technology Committee TC-31FS.

Normative text is text that describes elements of the design that are indispensable or contains the conformance language keywords: “shall”, “should”, or “may”. Informative text is text that is potentially helpful to the user, but not indispensable, and can be removed, changed, or added editorially without affecting interoperability. Informative text does not contain any conformance keywords.

All text in this document is, by default, normative, except: the Introduction, any section explicitly labeled as “Informative” or individual paragraphs that start with “Note:”

The keywords “shall” and “shall not” indicate requirements strictly to be followed in order to conform to the document and from which no deviation is permitted. The keywords “should” and “should not” indicate that, among several possibilities, one is recommended as particularly suitable, without mentioning or excluding others; or that a certain course of action is preferred but not necessarily required; or that (in the negative form) a certain possibility or course of action is deprecated but not prohibited.

The keywords “may” and “need not” indicate courses of action permissible within the limits of the document.

The keyword “reserved” indicates a provision that is not defined at this time, shall not be used, and may be defined in the future. The keyword “forbidden” indicates “reserved” and in addition indicates that the provision will never be defined in the future.

A conformant implementation according to this document is one that includes all mandatory provisions (“shall”) and, if implemented, all recommended provisions (“should”) as described. A conformant implementation need not implement optional provisions (“may”) and need not implement them as described. Unless otherwise specified, the order of precedence of the types of normative information in this document shall be as follows: Normative prose shall be the authoritative definition; Tables shall be next; then formal languages; then figures; and then any other language forms.

If this is a revision, a topical list of changes [should/shall be included here]

# Introduction

An Introduction section is Optional / Conditional

The introduction provides specific information or commentary about the technical content of the document, and about the reasons prompting its preparation. See AG-16 clause 3.3 (Introduction), AG-16 clause 4.2 (Conformance Terms), and ISO Directive Part 2 clause 13 (Introduction).

This section is entirely informative and does not form an integral part of this Engineering Document.

SMPTE ST 2117-1 (VC-6) is a versatile compression intra-frame scheme. This document maps the VC-6 bitstream into the MXF Generic Container. The usage of this mapping to synchronise with other components such as audio and video is outside the scope of this document.

The MXF Generic Container is a streamable Essence Container that can be placed on any suitable transport and stored. SMPTE ST 379-1 defines the MXF Generic Container as the native Essence Container in MXF files. SMPTE ST 379-2 defines the MXF Constrained Generic Container.

Other MXF mapping documents such as SMPTE ST 382 define how Audio can be mapped and synchronised with the video stream in the MXF Generic Container.

[Editors notes: The following paragraph will be replaced with the appropriate patent information during the SMPTE Headquarters publication process.]

At the time of publication, no notice had been received by SMPTE claiming patent rights essential to the implementation of this Engineering Document. However, attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. SMPTE shall not be held responsible for identifying any or all such patent rights.

# 1 Scope

The scope clearly defines the subject of the document and the aspects covered, thereby indicating the limits of applicability of the document. See AG-16 clause 3.4 (Scope), and ISO Directive Part 2 clause 14 (Scope).

This Standard constrains the MXF mapping of SMPTE ST-2117-1 into the MXF Generic Container or MXF Constrained Generic Container.

# 2 Normative References

The normative references clause lists, for information, those documents which are cited normatively in the document. See AG-16 clause 3.5 (Normative References), AG-16 clause 4.3 (Normative References to Standards and Recommended Practices), and the ISO Directives Clause 15 (Normative References).

The following SMPTE STANDARD contains provisions that, through reference in this text, constitute provisions of this standard. [Dated references require that the specific edition cited shall be used as the reference. Undated citations refer to the edition of the referenced document (including any amendments) current at the date of publication of this document. All SMPTE STANDARD are subject to revision, and users of this engineering document are encouraged to investigate the possibility of applying the most recent edition of any undated reference.

SMPTE ST 326:2000, Television — SDTI Content Package Format (SDTI-CP)

SMPTE ST 331:2011, Element and Metadata Definitions for the SDTI-CP

SMPTE ST 377-1:2019, Material Exchange Format (MXF) — File Format Specification

SMPTE ST 378:2004, Television — Material Exchange Format (MXF) — Operational pattern 1A (Single Item, Single Package)

SMPTE ST 379-1:2009, Material Exchange Format (MXF) — MXF Generic Container

SMPTE ST 379-2:2010, Television — Material Exchange Format (MXF) — MXF Constrained Generic Container

SMPTE ST 381-2:2011, Material Exchange Format (MXF) — Mapping MPEG Streams into the MXF Constrained Generic Container

SMPTE ST 382:2007, Material Exchange Format — Mapping AES3 and Broadcast Wave Audio into the MXF Generic Container

SMPTE ST 385:2012, Material Exchange Format (MXF) — Mapping SDTI-CP Essence and Metadata into the MXF Generic Container

SMPTE ST 400:2012, SMPTE Labels Structure

SMPTE ST 436-1:2013, MXF Mappings for VI Lines and Ancillary Data Packet

# 3 Terms and Definitions

The terms and definitions clause provide definitions necessary for the understanding of certain terms used in the document. See AG-16 clause 3.6 (Terms and Definitions), AG-16 clause 4.4 (Terms and Definitions), and ISO Directive Part 2 clause 16 (Terms and Definitions).

Select one of the following sentences and delete the others:

a) For the purposes of this document, the following terms and definitions apply:

b) For the purposes of this document, the terms and definitions given in [external reference(s)] apply.

c) For the purposes of this document, the terms and definitions given in [external reference(s)] and the following apply:

d) No terms and definitions are listed in this document.

If sentence b) or d) is selected, nothing else appears in the Clause.

If sentence a) or c) is selected, one or more terms is defined in the clauses immediately following.

Your terms and definitions follow.

All Terms and Definitions are defined in SMPTE ST 377-1 and SMPTE ST 379-2.

# 4 MXF File Structure and Mapping

## 4.1 General

SMPTE ST-2117-1, MXF files specified by this document shall have one of the two structures illustrated in Figure 1 and Figure 2 respectively. **HPP** is an apbbrivciation for Header Partition Pack, **BPP** is an abbreviation for Body Partition Pack and **FPP** is a shorthand for Footer Partition Pack.

Figure 1 - Single Essence Location Style

Figure 1 - Single Essence Location Style

Figure 2 - Multiple Essence Location Style

Figure 2 - Multiple Essence Location Style

Detailed constraints are listed in Annex B Constraints of a Conformant Implementation.

## 4.2 Single Essence Location Style

As shown in Figure 1, this style consists of a Header Partition, a Footer Partition, and a Random Index Pack.

The Index Table is placed prior to the Essence Container.

Some of the aspects of this style are shown below.

* It is easy to handle because of a simple structure
* It is easy to edit while file transferring
* It is easy to pick extract a “Partial file”

The following Index Layout Properties shall be set according to SMPTE ST 377-1.

* Index Table Segment::Single Index Location TRUE (Single Location)
* Index Table Segment::Single Location TRUE (Single Location)
* Index Table Segment::Forward Index Direction TRUE (Forward)
* Preface:: is RIP present TRUE

## 4.3 Multiple Essence Location Style

As shown in Figure 2, this style consists of a Header Partition, segmented Body Partition(s), a Footer Partition, and a Random Index Pack. Every Body Partition carrying VC-6 data shall be followed by one Index Table Segment that carries the Index Entries for the Edit Units of that Body Partition.

Some of the aspects of this style are shown below

* It is only necessary to include one Index Table Segment for each Body Partition period on the sender side
* It is easy to perform the function “Play while receiving file” on the receiver side
* It is easy to pick extract a “Partial file”

The following Index Layout Properties shall be set according to SMPTE ST 377-1.

* Index Table Segment::Single Index Location FALSE (Distributed Location)
* Index Table Segment::Single Essence Location FALSE (Distributed Location)
* Index Table Segment::Forward Index Direction FALSE (Backward)
* Preface:: is RIP present TRUE
* Essence Container Data:: Following Index Table TRUE (A Complete Index Table follows all Essence)

# 5 Mapping VC-6 Bytestream into the MXF Gegneric Container

HEVC streams shall be mapped using the MXF Generic Container using frame wrapping as defined in SMPTE ST 379-1 and SMPTE ST 379-2

Figure 4 shows the SMPTE ST-2117 picture element, the byte stream shall comply with SMPTE ST-2117.

Mapping of ST-2117 Picture Item Element

Mapping of ST-2117 Picture Item Element

# 6 Key Length Value Encoding

## 6.1 Picture Element Key

### 6.1.1 SMPTE ST-2117 Picture Element Key

Table 1

|  |  |  |  |
| --- | --- | --- | --- |
| Item Name | Symbol | Kind | Item UL |
| Frame Wrapped VC6 Picture Element | FrameWrappedVC6PictureElement | LEAF | urn:smpte:ul:060E2B34.01020101.0D010301.15kk05nn |

The parameter kk specifies the count of Picture Elements in the Picture Item, and nn indicates the index number of the Element. For VC-6 mappings kk should have the value 01 and nn should have the value 01.

### 6.1.2 SMPTE ST-2117 Picture Element Length

The length field of the KLV coded Element shall be 4 bytes BER long-form encoded (i.e. 83h.xx.yy.zz).

### 6.1.3 SMPTE ST-2117 Picture Element Value

Each Picture Element shall be a byte stream for a single image compliant with SMPTE ST-2117-1.

# 7 MXF Labels

## 7.1 Essence Container Label

The Essence Container Label is carried in the Essence Containers Properties of the Partition Packs, Preface Set and File Descriptor.

The values of the Essence Container Label for VC-6 Bytestreams in MXF shall be on eof the values in Table 2.

Table 2 – Essence Container Label Values for HEVC

|  |  |  |  |
| --- | --- | --- | --- |
| Item Name | Symbol | Kind | Item UL |
| VC6 Generic Bytestream | VC6GenericBytestream | LEAF | urn:smpte:ul:060E2B34.01020101.0D010301.15kk05nn |

## 7.2 Picture Essence Coding Label

The Picture Essence Coding Label is used in the Generic Picture Essence Descriptor. The values for the Picture Essence Coding Label for the HEVC are given in Table 3. These Label values are listed in the SMPTE Labels Register.

Table 3 – Picture Essence Coding Label Values for HEVC

|  |  |  |  |
| --- | --- | --- | --- |
| Item Name | Symbol | Kind | Item UL |
| VC6 Generic Bytestream | VC6GenericBytestream | LEAF | urn:smpte:ul:060E2B34.01020101.0D010301.15kk05nn |

**Information for Document Editors (this page is to be deleted prior to FCD ballot)**

The following documents have useful reference material for document editors. SMPTE AG 16:2018 – SMPTE Engineering Document Style Guidelines

International Organization for Standardization (ISO) / International Electrotechnical Commission (IEC), Directives, Part 2:2016-05, Principles and rules for the structure and drafting of ISO and IEC documents, 7.0

**Warning**: Only copy-and-paste plain text from other documents; otherwise this style set may be corrupted.

The refdoc for this document type is in the refdocs folder of this project. It explains how the types work.

If you extend the document types with your own refdoc, the **YOU MUST** make Home Office aware, otherwise the styles may be lost.